**12000 GVWR Low Profile**



GVWR: 12,000 lb.  
Capacity: 8,400 lb.

* Two 6,000 lb. Dexter Brand Braking Axles
* Double Eye Spring Suspension
* 235/80 R16 Load Range E10 Ply Rating Westlake Radial Tires
* 6″ Channel Main Frame – 6″ Channel Tongue
* 3×3 Tubing Dump Box Frame With 3″ Channel Cross Members
* 12 Gauge Floor
* 80″ Inside Box With 24″ Sides And No Stick Bottom Corners
* US Made Pump With Deep Cycle Battery Inside Lockable Security Box With 20′ Hand Remote
* Two Way Tailgate Opens For Dumping Bulk Materials Or Can Be Set In Spreader Mode
* 80″ 3″ Channel Slide-In Loading Ramps
* 2 5/16″ Adjustable Coupler
* 7,000 lb. Drop Foot Jack
* Safety Chains And Break-a-Way Switch
* LED Lighting With Reflective Tape
* Primed with epoxy primer and two coats of polyurethane paint
* [AVAILABLE SIZES](https://hawketrailers.com/hawke-dump-trailers/low-profile-dump-trailers/12000-gvwr-low-profile/#tab-1)

**Available Sizes**

* 80″ x 12′ – Empty Weight 3,400 lb.
* 80″ x 14′ – Empty Weight 3,600 lb.